# **Seco South LED System Light:**

# **S33-WC00-1**

By Tecniq

Specifications include:

a.            Lamp Type:

                ¾” grommet mounted white light with 90 degree output

b.            Light Illumination:

                White 65 lumens (available in turtle friendly amber)

c.            Efficacy:

                63.5%

d.            Color Rendering Index: Minimum [**65**] [**70**] [**80**] <**Insert number**>.

                80+

e.             Correlated Color Temperature:

                5000K

f.            Rated Lamp Life:

                50,000 hours

g.            Beam Distribution:

1. degree cone

h. LED Diffuser:

              Polycarbonate

I.             Nominal Operating Voltage:

12v

J.            Internal Driver:

   Resistor based

L. Listing:

            IP68 Rated. Completely Sealed, Water proof design.

M.. Draw:

            .06 - .08A and its .96wat per light

O. Mounting:

            Gasket with 316 stainless steel beauty ring.